
AdapterId 0FFAFh

AdapterName "Built In Features"

NumBytes 1

FixedResources
        pos[0]=XXXXXX11b io 03f0h-03f7h  int 6
                                         arb 2
                                         mem 0fffe0000h - 0ffffffffh

sysmem 1024

NamedItem Prompt "Serial Port"
        choice "SERIAL_1"  pos[0]=XXXX11XXb  io 03f8h-03ffh  int 4
        choice "SERIAL_2"  pos[0]=XXXX01XXb  io 02f8h-02ffh  int 3
        choice "Disabled"  pos[0]=XXXX10XXb

        Help
        "The built-in serial port connector can be assigned as Serial
        1, Serial 2, or disabled.  Use the F5=Previous and the F6=Next keys to
        change serial port assignments if you are in the 'Change
        configuration' window.  Conflicting assignments are marked
        with an asterisk and should be changed."

NamedItem Prompt "Parallel Port"
        choice "PARALLEL_1"  pos[0]=1001XXXXb  io 03bch-03bfh
        choice "PARALLEL_2"  pos[0]=1011XXXXb  io 0378h-037bh
        choice "PARALLEL_3"  pos[0]=1101XXXXb  io 0278h-027bh
        choice "Disabled"    pos[0]=1000XXXXb

        Help
        "The built-in parallel port connector can be assigned
        as Parallel 1 through Parallel 3 or disabled.  Use the F5=Previous
        and the F6=Next keys to change parallel port assignments if you
        are in the 'Change configuration' window.  Conflicting assignments
        are marked with an asterisk and should be changed."
