AdapterId 07051h

AdapterName "AST RampagePlus/MC With I/O Pak/MC-S Option"

NumBytes 4

NamedItem
   Prompt "Wait State"
      choice "1 wait state " pos[1]=0XXXXXXXb
      choice "0 wait state " pos[1]=1XXXXXXXb
   Help
      "Memory WAIT STATE selection"

NamedItem
   Prompt "Memory Configuration"
      choice "DISABLED"   pos[0]=1010000Xb
      choice ".5M,0K,0K,0K    TOTAL = 0.5 MB" pos[0]=1111001Xb
      choice ".5M,.5M,0K,0K   TOTAL = 1.0 MB" pos[0]=1110001Xb
      choice ".5M,.5M,.5M,0K  TOTAL = 1.5 MB" pos[0]=1101001Xb
      choice ".5M,.5M,.5M,.5M TOTAL = 2.0 MB" pos[0]=1100001Xb
      choice " 2M,0K,0K,0K    TOTAL = 2.0 MB" pos[0]=1001001Xb
      choice ".5M,2M,0K,0K    TOTAL = 2.5 MB" pos[0]=0110001Xb
      choice ".5M,.5M,2M,0K   TOTAL = 3.0 MB" pos[0]=0101001Xb
      choice ".5M,.5M,.5M,2M  TOTAL = 3.5 MB" pos[0]=0100001Xb
      choice " 2M,2M,0K,0K    TOTAL = 4.0 MB" pos[0]=1000001Xb
      choice ".5M,2M,2M,0K    TOTAL = 4.5 MB" pos[0]=0011001Xb
      choice ".5M,.5M,2M,2M   TOTAL = 5.0 MB" pos[0]=0111001Xb
      choice " 2M,2M,2M,0K    TOTAL = 6.0 MB" pos[0]=0001001Xb
      choice ".5M,2M,2M,2M    TOTAL = 6.5 MB" pos[0]=0010001Xb
      choice " 2M,2M,2M,2M    TOTAL = 8.0 MB" pos[0]=0000001Xb
   Help
"This is memory configuration on your RampagePlus/MC
starting from top of the board BANK0,BANK1,BANK2,BANK3"

NamedItem
     Prompt "Connector 1"
        choice "SERIAL_1"
                      pos[2]=XXXX0001b
                      io 03f8h-03ffh int 4
        choice "SERIAL_2"
                      pos[2]=XXXX0011b
                      io 02f8h-02ffh int 3
        choice "SERIAL_3"
                      pos[2]=XXXX0101b
                      io 3220h-3227h int 3
        choice "SERIAL_4"
                      pos[2]=XXXX0111b
                      io 3228h-322fh int 3
        choice "SERIAL_5"
                      pos[2]=XXXX1001b
                      io 4220h-4227h int 3
        choice "SERIAL_6"
                      pos[2]=XXXX1011b
                      io 4228h-422fh int 3
        choice "SERIAL_7"
                      pos[2]=XXXX1101b
                      io 5220h-5227h int 3
        choice "SERIAL_8"
                      pos[2]=XXXX1111b
                      io 5228h-522fh int 3
        choice "DISABLE"
                      pos[2]=XXXXXXX0b
     Help
        "Connector 1 of the RampagePlus/MC with I/O Pak/MC-S
        (Dual  Serial Port)  Option  can have  any one  of the
        Serial 1  to  Serial 8  assignments  and  can also  be
        disabled.  Use the F5 = Previous and F6 = Next keys to
        change the Connector 1 Serial Port assignment when you
        are in the 'Change Configuration' window.  Conflicting
        assignments  are marked with an asterisk and should be
        changed."

NamedItem
     Prompt "Connector 2"
        choice "SERIAL_2"
                      pos[2]=0011XXXXb
                      io 02f8h-02ffh int 3
        choice "SERIAL_3"
                      pos[2]=0101XXXXb
                      io 3220h-3227h int 3
        choice "SERIAL_4"
                      pos[2]=0111XXXXb
                      io 3228h-322fh int 3
        choice "SERIAL_5"
                      pos[2]=1001XXXXb
                      io 4220h-4227h int 3
        choice "SERIAL_6"
                      pos[2]=1011XXXXb
                      io 4228h-422fh int 3
        choice "SERIAL_7"
                      pos[2]=1101XXXXb
                      io 5220h-5227h int 3
        choice "SERIAL_8"
                      pos[2]=1111XXXXb
                      io 5228h-522fh int 3
        choice "DISABLE"
                      pos[2]=XXX0XXXXb
     Help
        "Connector 2 of the RampagePlus/MC with I/O Pak/MC-S
        (Dual  Serial Port)  Option  can have  any one  of the
        Serial 1  to  Serial 8  assignments  and  can also  be
        disabled.  Use the F5 = Previous and F6 = Next keys to
        change the Connector 2 Serial Port assignment when you
        are in the 'Change Configuration' window.  Conflicting
        assignments  are marked with an asterisk and should be
        changed."
