
AdapterId 06786h

AdapterName  "NeoTecH DP/1A, two channel parallel adapter"

NumBytes 1

NamedItem
        Prompt "Parallel Ports,  see model 80 notes"       
      choice "Parallel_2/3"   pos[0]=XXXXX011b  io 0378H-037AH 
                                                   0278H-027AH  int 7
      choice "Parallel_1/2"   pos[0]=XXXXX111b  io 03BCH-03BEh
                                                   0378H-037AH  int 7
      choice "Parallel_1/3"   pos[0]=XXXXX101b  io 03BCH-03BEH
                                                   0278H-027AH  int 7      
   Help
   "LPT assignments are determined by the BIOS POST function
    and do not necessarily correspond to the parallel port assignments.
    PS/2 models 80-A21 and 80-A31 differ from most PS/2's. For more
    information remove the DP/1A, return to your operating system, insert
    the installation diskette and type LPTINFO <enter>."
