
AdapterId 06222h

AdapterName "The NCI 4700 PCI/MC"

NumBytes 3

FixedResources
         pos[0]=XXXXXXXXb
         pos[2]=1X000110b
         io 0220h-022Fh 02D0h-02DFh
         int 2
         mem 0CC000h-0CFFFFh

NamedItem

    Prompt "Adapter Feature selection"
         Choice "REMOTE IPL"
              pos[1]=XXXXXXX1b
         Choice "LOCAL IPL"
              pos[1]=XXXXXXX0b

    Help
         "You must choose the adapter features you wish to run with.
         REMOTE IPl means to Boot the system from the 4702.
         LOCAL IPL means to Boot the system from the local hard disk."

NamedItem

    Prompt "Adapter Feature selection"
         Choice "DISKETTE ENABLE"
              pos[1]=XXXXXX0Xb
         Choice "DISKETTE DISABLE"
              pos[1]=XXXXXX1Xb

    Help
         "You must choose the adapter features you wish to run with.
         DISKETTE ENABLE means that the diskette drives are available if
         present.
         DISKETTE DISABLE means the diskette drives are disabled and
         not available to be used."

NamedItem

    Prompt "Adapter Feature selection"
         Choice "PRIMARY DOS"
              pos[1]=XXXXX1XXb
         Choice "SECONDARY DOS"
              pos[1]=XXXXX0XXb

    Help
         "You must choose the adapter features you wish to run with.
         PRIMARY DOS means to boot the system as if there were no dual
         DOS system. SECONDARY DOS means to boot the system from the
         secondary DOS system on the remote reset volume."

NamedItem

    Prompt "Adapter Feature selection"
         Choice "IPL OVERRIDE"
              pos[1]=XXXX1XXXb
         Choice "NO IPL OVERRIDE"
              pos[1]=XXXX0XXXb

    Help
         "You must choose the adapter features you wish to run with.
         IPL OVERRIDE means that the operator may choose
         an alternanate IPL by pressing F1. NO IPL OVERRIDE means that
         no override of the ipl device is possible."


