; CuModem 2400 Baud Modem 
; Copyright (c) Cumulus Corporation 1987. All rights reserved

AdapterId 7026h

AdapterName "Cumulus 2400 Baud Internal Modem"

Numbytes 3

NamedItem

	Prompt "Serial Port autoselected at "

	choice "COM1 configuration"
		pos[0]=xxx001xxb
		io 3f8h - 3ffh
		int 4

	choice "COM2 configuration"
		pos[0]=xxx011xxb
		io 2f8h - 2ffh
		int 3	

	choice "COM3 configuration"
		pos[0]=xxx101xxb
		io 3220h - 3227h
		int 3

	choice "COM4 configuration"
		pos[0]=xxx111xxb
		io 3228h - 322fh
		int 3

	choice 	"Disable Serial Port"
		pos[0]=xxxxx0xxb

	Help
	" Use the F5 or F6 key to select desired COM port"

