
AdapterId 06e78h

AdapterName "IRMA2 Adapter"

NumBytes 1 

NamedItem
        Prompt "DCA 3270 Adapter For PS2"
      choice "220h-22Fh,280h-29Fh"    pos[0]=xxx1000xb  io 0220h-022Fh 0280h-029Fh
      choice "280h-29Fh"    pos[0]=xxx1001xb  io 0280h-029Fh
      choice "2C0h-2DFh"    pos[0]=xxx1011xb  io 02C0h-02DFh
      choice "A80h-A9Fh"    pos[0]=xxx1101xb  io 0A80h-0A9Fh
      choice "AC0h-ADFh"    pos[0]=xxx1111xb  io 0AC0h-0ADFh

   Help
"This port can be assigned as Hex addresses 220h-22Fh & 280h-29Fh
(IRMA port enabled), 280h-29Fh, 2C0h-2DFh, A80h-A9Fh or AC0h-ADFh.
Use the F5=Previous and the F6=Next keys to change this assignment 
in the 'Change Configuration' window. Conflicting assignments
are marked with an asterisk and must be changed to use the adapter.
Rev IRMA2 v1.01"
