;
;	$Revision:   1.0  $
;	$Date:   21 Apr 1989  9:22:54  $
;
;***************************************************************************
;* Copyright (C) 1988 by Phoenix Technologies Ltd.  This program           *
;* contains proprietary and confidential information.  All rights reserved *
;* except as may be permitted by prior written consent.                    *
;***************************************************************************
; SYS00FF.ADF
; This file is used in conjunction with DFFD drives. Its supports the 
; entering of custom Hard Drive parameters in Extended CMOS 

; These three fields are irrelevant but must be present for the parser

AdapterId 00FFh
AdapterName "FF drive type"
NumBytes 0

;*************************************************************
;   Drive 0 information
;*************************************************************

NamedItem
Prompt "Drive 0 - Number of tracks   "
ECmos2 166h
Numeric 1-1024
Choice " 10" pos[0]=XXXXXXXXb
Help
"Type in the number of tracks (cylinders) in the drive."

NamedItem
Prompt "          Number of heads    "
ECmos 168h
Numeric 1-100 
Choice " 10" pos[0]=XXXXXXXXb
Help
"Type in the number of heads in the drive."

NamedItem
Prompt "          Sectors per track  "
ECmos 174h
Numeric 1-100 
Choice " 10" pos[0]=XXXXXXXXb
Help
"Type in the number of sectors per track"

NamedItem
Prompt "          Landing Zone       "
ECmos2 172h
Numeric 0-1024 
Choice " 10" pos[0]=XXXXXXXXb
Help
"Type in the head landing zone for the drive."

NamedItem
Prompt "          Write Precomp      "
ECmos2 16bh
Numeric ffffffffh-1024d 
Choice " 10" pos[0]=XXXXXXXXb
Help
"Type in the Starting Write Precompensation Cylinder for the drive. 
Use -1 if no Precomp is required."

NamedItem
Prompt "          Defect Map         "
ECmos 16eh
Choice "Yes" pos[0]=XX10X000b
Choice "No " pos[0]=XX00X000b
Help
"Select Yes if the drive supports Defect Maps."

NamedItem
Prompt "          More than 8 heads  "
ECmos 16eh
Choice "No " pos[0]=XXX00000b
Choice "Yes" pos[0]=XXX01000b
Help
" Select Yes if the drive has more than 8 heads. This setting must
be consistent with the 'Number of heads' choice."

NamedItem
Prompt "          Disable retries    "
ECmos 16eh
Choice "No " pos[0]=00X0X000b
Choice "Yes" pos[0]=11X0X000b
Help
" Select No if the drive supports retries."

NamedItem
Nodisplay
Prompt "Drive 0-extended drive table"
Cmos 11h
Choice "Yes" pos[0]=11111111b
Help
"This selection must always be set to hex FF."





