AdapterId 06040h
AdapterName "Intel 2400B Modem 2"
NumBytes 1
NamedItem

        Prompt "Modem Serial Port Address"
    choice "SERIAL_1" pos[0]=XXXX000Xb io 03f8h-03ffh int 4
    choice "SERIAL_2" pos[0]=XXXX001Xb io 02f8h-02ffh int 3
    choice "SERIAL_3" pos[0]=XXXX010Xb io 3220h-3227h int 3
    choice "SERIAL_4" pos[0]=XXXX011Xb io 3228h-322fh int 3
    choice "SERIAL_5" pos[0]=XXXX100Xb io 4220h-4227h int 3
    choice "SERIAL_6" pos[0]=XXXX101Xb io 4228h-422fh int 3
    choice "SERIAL_7" pos[0]=XXXX110Xb io 5220h-5227h int 3

Help "The Intel 2400B Modem 2 may be assigned to use SERIAL_1 through
Serial_7.  Use F5 to select the previous address port, and F6
to select the next if you are in the 'Change Configuration' window.
Conflicting assignments are marked with an asterisk (*) and must be
changed before you can use the Modem."
