
AdapterID 07048h

AdapterName  "EXCELOGIC MICROMEM BOARD"

NumBytes 2

fixedresources
        pos[1]=00000000b
initprog 30

nameditem
        Prompt  "RAM installed before this card: "

          Choice "1  MEG of RAM"
            pos[0]=00000100b

          Choice "1.5 MEG of RAM"
            pos[0]=00000110b

          Choice "2  MEG of RAM"
            pos[0]=00001000b

          Choice "2.5 MEG of RAM"
            pos[0]=00001010b

          Choice "3  MEG of RAM"
            pos[0]=00001100b

          Choice "3.5 MEG of RAM"
            pos[0]=00001110b

          Choice "4  MEG of RAM"
            pos[0]=00010000b

          Choice "4.5 MEG of RAM"
            pos[0]=00010010b

          Choice "5  MEG of RAM"
            pos[0]=00010100b

          Choice "5.5 MEG of RAM"
            pos[0]=00010110b

          Choice "6  MEG of RAM"
            pos[0]=00011000b

          Choice "6.5 MEG of RAM"
            pos[0]=00011010b

          Choice "7  MEG of RAM"
            pos[0]=00011100b

          Choice "7.5 MEG of RAM"
            pos[0]=00011110b

         Choice "8  MEG of RAM"
            pos[0]=00100000b

          Choice "8.5 MEG of RAM"
            pos[0]=00100010b

         Choice "9  MEG of RAM"
            pos[0]=00100100b

          Choice "9.5 MEG of RAM"
            pos[0]=00100110b

         Choice "10  MEG of RAM"
            pos[0]=00101000b

          Choice "10.5 MEG of RAM"
            pos[0]=00101010b

          Choice "11  MEG of RAM"
            pos[0]=00101100b

          Choice "11.5 MEG of RAM"
            pos[0]=00101110b

          Choice "12  MEG of RAM"
            pos[0]=00110000b

          Choice "12.5 MEG of RAM"
            pos[0]=00110010b

          Choice "13  MEG of RAM"
            pos[0]=00110100b

          Choice "13.5 MEG of RAM"
            pos[0]=00110110b

          Choice "14  MEG of RAM"
            pos[0]=00111000b

          Choice "14.5 MEG of RAM"
            pos[0]=00111010b

          Choice "15  MEG of RAM"
            pos[0]=00111100b

          Choice "15.5 MEG of RAM"
            pos[0]=00111110b

          Choice "Card Disable (Not Used)"
            pos[0]=00000000b

        Help
        "To configure this adapter you must choose to have it enabled or  
         disabled."
