
AdapterId 06783h

AdapterName  "NEOTECH SERIAL/PARALLEL ADAPTER"

NumBytes 1

NamedItem
        Prompt "COMx/LPTx"       
      choice "SERIAL2/LPT2"  pos[0]=1XXXXX01b  io 02F8h-02FFh  int 3
      choice "SERIAL3/LPT3"  pos[0]=1XXXXX11b  io 3220h-3227h  int 3
   Help
"This allows you to set this card to either COM2 or COM3. 
 Use the F5=Previous and the F6=Next keys to change serial port
 assignments if you are in the 'Change configuration' window.
 Conflicting assignments are marked with an asterisk and
 must be changed to use the adapter."
