
AdapterId 0E3FFh

AdapterName "Built In Features"

NumBytes 1

FixedResources
	pos[0]=XXXXXX11b io 03f0h-03f7h  int 6
					 arb 2
					 mem 0fe0000h - 0ffffffh

sysmem 1024
Begin
NamedItem Prompt "Serial Port"
	choice "SERIAL_1"  pos[0]=XXXX11XXb  io 03f8h-03ffh  int 4
	choice "SERIAL_2"  pos[0]=XXXX01XXb  io 02f8h-02ffh  int 3
	choice "Disabled"  pos[0]=XXXX10XXb

	Help
	"The built-in serial port connector can be assigned as Serial
	1, Serial 2, or disabled.  Use the F5=Previous and the F6=Next keys to
	change serial port assignments if you are in the 'Change
	configuration' window.  Conflicting assignments are marked
	with an asterisk and should be changed."
End
Begin
NamedItem Prompt "Parallel Port"
	choice "PARALLEL_1"  pos[0]=1001XXXXb  io 03bch-03bfh
	choice "PARALLEL_2"  pos[0]=1011XXXXb  io 0378h-037bh
	choice "PARALLEL_3"  pos[0]=1101XXXXb  io 0278h-027bh
	choice "Disabled"    pos[0]=1000XXXXb

	Help
	"The built-in parallel port connector can be assigned
	as Parallel 1 through Parallel 3 or disabled.  Use the F5=Previous
	and the F6=Next keys to change parallel port assignments if you
	are in the 'Change configuration' window.  Conflicting assignments
	are marked with an asterisk and should be changed."
End
