AdapterId 07050h

AdapterName  "AST RampagePlus/MC"

NumBytes 4

NamedItem
   Prompt "Wait State"
      choice "1 wait state " pos[1]=0XXXXXXXb
      choice "0 wait state " pos[1]=1XXXXXXXb
   Help
      "Memory WAIT STATE selection"

NamedItem
   Prompt "Memory Configuration"
      choice "DISABLED"   pos[0]=1010000Xb
      choice ".5M,0K,0K,0K    TOTAL = 0.5 MB" pos[0]=1111001Xb
      choice ".5M,.5M,0K,0K   TOTAL = 1.0 MB" pos[0]=1110001Xb
      choice ".5M,.5M,.5M,0K  TOTAL = 1.5 MB" pos[0]=1101001Xb
      choice ".5M,.5M,.5M,.5M TOTAL = 2.0 MB" pos[0]=1100001Xb
      choice " 2M,0K,0K,0K    TOTAL = 2.0 MB" pos[0]=1001001Xb
      choice ".5M,2M,0K,0K    TOTAL = 2.5 MB" pos[0]=0110001Xb
      choice ".5M,.5M,2M,0K   TOTAL = 3.0 MB" pos[0]=0101001Xb
      choice ".5M,.5M,.5M,2M  TOTAL = 3.5 MB" pos[0]=0100001Xb
      choice " 2M,2M,0K,0K    TOTAL = 4.0 MB" pos[0]=1000001Xb
      choice ".5M,2M,2M,0K    TOTAL = 4.5 MB" pos[0]=0011001Xb
      choice ".5M,.5M,2M,2M   TOTAL = 5.0 MB" pos[0]=0111001Xb
      choice " 2M,2M,2M,0K    TOTAL = 6.0 MB" pos[0]=0001001Xb
      choice ".5M,2M,2M,2M    TOTAL = 6.5 MB" pos[0]=0010001Xb
      choice " 2M,2M,2M,2M    TOTAL = 8.0 MB" pos[0]=0000001Xb
   Help
"This is memory configuration on your RampagePlus/MC
starting from top of the board BANK0,BANK1,BANK2,BANK3"
