
AdapterId 06781h

AdapterName  "NEOTECH SERIAL ADAPTER"

NumBytes 1

NamedItem
        Prompt "COMn"       
      choice "SERIAL2"  pos[0]=XXXXXX01b  io 02F8h-02FFh  int 3
      choice "SERIAL3"  pos[0]=XXXXXX11b  io 3220h-3227h  int 3
   Help
"This allows you to set this card to either COM2 or COM3. 
 Use the F5=Previous and the F6=Next keys to change serial port
assignments if you are in the 'Change configuration' window.
Conflicting assignments are marked with an asterisk and
must be changed to use the adapter."
