
AdapterId 0601Fh

AdapterName "Hewlett-Packard Scanner Interface Adapter"

NumBytes 1

FixedResources 
	pos[0]=1XXXXXXXb int 7

NamedItem
	Prompt "I/O Port Location"
		choice "278-27FH (PARALLEL_3)"  pos[0]=X11XXXXXb io 0278h-027Fh
		choice "268-26FH"  pos[0]=X10XXXXXb io 0268h-026Fh
		choice "258-25FH"  pos[0]=X01XXXXXb io 0258h-025Fh
		choice "248-24FH"  pos[0]=X00XXXXXb io 0248h-024Fh
	Help
	"This adapter requires eight I/O ports.  There are four choices for the
	 location of these ports.  Normally choice [278-27FH] will be fine.  
	 However, if you already have a parallel port configured as Parallel 
	 port 3, or some other adapter that uses these locations there will be 
	 a conflict (indicated by an asterisk).  Use the F5=Previous and F6=Next 
	 keys while in the Change Configuration display to find a choice that 
	 does not conflict with other adapters in the system (the asterisk will 
	 go away)."

NamedItem
	Prompt "Memory Location"
		choice "Segment C400" pos[0]=XXX1001Xb mem 0C4000h - 0C7FFFh
		choice "Segment CC00" pos[0]=XXX1011Xb mem 0CC000h - 0CFFFFh
		choice "Segment DC00" pos[0]=XXX1111Xb mem 0DC000h - 0DFFFFh
		choice "Segment D800" pos[0]=XXX1110Xb mem 0D8000h - 0DBFFFh
		choice "Segment D400" pos[0]=XXX1101Xb mem 0D4000h - 0D7FFFh
		choice "Segment D000" pos[0]=XXX1100Xb mem 0D0000h - 0D3FFFh
		choice "Segment C000" pos[0]=XXX1000Xb mem 0C0000h - 0C3FFFh
		choice "Segment C800" pos[0]=XXX1010Xb mem 0C8000h - 0CBFFFh
	Help
	"This adapter requires 16 Kbytes of memory space from the adapter ROM
         area.  There are eight memory locations that can be selected.  Under
         normal conditions, [Segment C400] will be fine.  If there is a 
         conflict (indicated by an asterisk), select another segment using the
         F5=Previous and F6=Next keys while in the Change Configuration display 
	 until the asterisk goes away."
